## Strings

    "foo \"bar\" baz"
    'foo \'bar\' baz'
    "Multi-line strings ending with a \
    are supported too."

## Macro statements

    #include <Bridge.h>
    #define SOME_PIN 11

## Booleans

    true;
    false;

## Operators

    a < b;
    c && d;

## Full example

    #include <Bridge.h>

    // pin of the piezo speaker
    int piezo = 8;

    /**
     * setups
     * runs once before everyhing else
     */
    void setup() {
        pinMode(piezo, OUTPUT);
    }

    /**
     * loop
     * this will run forever and do what we want
     */
    void loop() {
        playMelody(1);
        delay(1000);
    }

    /**
     * playMelody
     * will play a simple melody on piezo speaker
     */
    void playMelody(int times) {
        int melody[] = { 4699, 4699, 3520, 4699 };
        int duration = 6;

        for( int t = 0; t < times; t++ ) {
            for( int i = 0; i < 4; i++ ) {
                // pass tone to selected pin
                tone(piezoPin, melody[i], 1000/duration);

                // get a bit of time between the tones
                delay(1000 / duration * 1.30 + 80);

                // and don't forget to switch of the tone afterwards
                noTone(piezoPin);
            }
        }
    }